Tile e094n20
Location (Lat,Long): 20°N, 94°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 46
Tile center (UTM: X,Y): 604609.32383, 2211793.55617 m
Upper left corner (UTM: X,Y): 594589.32383, 2221813.55617 m
Lower right corner (UTM: X,Y): 614629.32383, 2201773.55617 m

Landsat platform/sensor: 4/TM
WRS2 Path: 134; Row: 046
Date: 1989/01/23
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 5.657 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 60 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e094n20.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
